**Product Instructions**

**Client:**

1. Press the button for about 3 seconds
2. If you felt vibration, let go of the button
3. The server is now notified

**Server:**

1. Check for notification from the client if the red LED is blinking and/or the buzzer is buzzing.
2. Read the cup address shown on the screen.
3. If client’s concern has already been fixed, press the button once to return
4. In case of multiple clients sending notification at the same time, just press the button for equal number of times to the number of clients notifying.